For 1990-2009 cars
Engine Controls Components
Cell 20: Engine Data Sensors
OBD II Symbol Description Notice
Handling ESD Sensitive Parts Notice
Handling ESD Sensitive Parts Notice

### Circuit Description

The engine coolant temperature (ECT) sensor is a thermistor. A thermistor is a resistor whose value varies with temperature. The ECT sensor resistance is high if the coolant temperature is cold. The sensor resistance is low if the coolant temperature is warm. The ECT sensor is wired in series with a fixed resistor in the powertrain control module (PCM). The PCM applies 5 volts to the ECT sensor. The PCM monitors the voltage across the ECT sensor and converts the voltage into a temperature reading. The PCM will receive a high voltage input if the coolant temperature is cold. The PCM will receive a low voltage input if the coolant temperature is warm.

### Conditions for Running the DTC

• | The ignition is ON.

• | The engine is running.

### Conditions for Setting the DTC

• | The ECT sensor signal indicates that the engine coolant temperature is greater than 119°C (246°F).

• | The above conditions are present for at least 0.5 seconds.

### Action Taken When the DTC Sets

• | The PCM illuminates the malfunction indicator lamp (MIL).

• | The PCM records the operating conditions at the time that the diagnostic fails. This information is stored in the Freeze Frame buffer.

• | The PCM enters the Fail-Safe Function and assumes the engine coolant temperature is 80°C (176°F) while stopping EGR, ISC, and A/C control. The PCM turns ON the engine cooling fan.

### Conditions for Clearing the DTC

• | The MIL turns off after 3 consecutive passing trips without a fault present.

• | A History DTC clears after 40 consecutive warm-up cycles without a fault.

• | Use the Clear DTC Information function, or disconnect the PCM battery feed in order to clear the DTC.

### Diagnostic Aids

Check for any of the following conditions:

• | Use the Temperature vs Resistance table in order to check the ECT sensor at various temperature levels, and evaluate the possibility of a shifted sensor. A shifted sensor could result in a driveability complaint. Refer to Temperature Versus Resistance .

• | The ECT sensor readings should steadily rise to about 95°C (203°F) after the engine is started. The readings should stabilize when the thermostat opens. Verify that the engine is not overheating and has not been operated under conditions which could create an overheating condition.

• | The engine cooling fan will turn ON when the DTC sets.

An intermittent complaint may be caused by a fault in the ECT sensor electrical circuit. Inspect the wiring harness and the components for any of the following conditions:

• | Backed out terminals

• | Incorrect mating of terminals

• | Broken electrical connector locks

• | Incorrectly formed terminals or damaged terminals

• | Faulty terminal-to-wire connections

• | Physical damage to the wiring harness

• | A broken wire inside the insulation

• | Corrosion of electrical connections, of splices, or of terminals

If DTC P0117 cannot be duplicated, the Freeze Frame data can be useful in determining the vehicle operating conditions when the DTC first set.

### Test Description

The numbers below refer to the step numbers in the Diagnostic Table.

1. The Powertrain OBD System Check prompts the technician to complete some basic checks and store the freeze frame data on the scan tool if applicable. This creates an electronic copy of the data taken when the fault occurred. The information is then stored in the scan tool for later reference.

2. This step checks the current ECT sensor reading.

3. This step determines if the fault is present.

4. This step determines if the fault is caused by a shorted signal return circuit or by a malfunctioning ECT sensor.

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Powertrain On-Board Diagnostic (OBD) System Check? | -- | Go to Step 2 | Go to Powertrain On Board Diagnostic (OBD) System Check
2 |

1. Turn ON the ignition, leaving the engine OFF.
2. Install a scan tool.
3. Observe the ECT parameter on the scan tool data list.

Is the ECT display at or greater than the specified value?

119°C (246°F)

Go to Step 4

Go to Step 3

3 |

1. Turn ON the ignition, leaving the engine OFF.
2. Clear the scan tool information.
3. Operate the vehicle within the Freeze Frame conditions as noted.

Is a DTC P0117 set?

--

Go to Step 4

Go to Diagnostic Aids

4 |

1. Disconnect the ECT sensor electrical connector.
2. Observe the ECT parameter on the scan tool.

Is the ECT display at or below the specified value?

-40°C (-40°F)

Go to Step 7

Go to Step 5

5 |

1. Turn OFF the ignition.
2. Disconnect the PCM electrical connectors.
3. Check the ECT sensor signal (input) circuit for a short to ground.

Is the ECT sensor signal circuit shorted to ground?

--

Go to Step 8

Go to Step 6

6 |

1. Check the ECT sensor ground circuit for a short to voltage.
2. Repair as necessary.

Was a repair necessary?

--

Go to Step 10

Go to Step 9

7 | Replace the ECT sensor. Refer to Engine Coolant Temperature Sensor Replacement . Is the action complete? | -- | Go to Step 10 | --
8 | Repair the ECT sensor signal (input) circuit. Is the action complete? | -- | Go to Step 10 | --
9 | Replace the PCM. Refer to Powertrain Control Module Replacement . Is the action complete? | -- | Go to Step 10 | --
10 |

1. Clear the scan tool information and road test the vehicle within the Freeze Frame conditions that set the DTC.
2. Review the scan tool data and check for DTCs. The repair is complete if no DTCs are stored.

Are any DTCs displayed on the scan tool?

--

Go to the Applicable DTC Table

System OK