For 1990-2009 cars

## Body Rear End Adjustment Specifications 2 Door

#### Sheet Metal Tolerances--2-Door Model

Location | Clearance Gap | Flushness
--- | --- | ---
Important: Use the following specifications in order to ensure the proper clearances and flushness of the rear end body components after body repair procedures are complete.
Front door to Quarter Panel (3) | 5.0 mm (0.20 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
Liftgate Door to Quarter Window (2) | 6.3 mm (0.25 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
Liftgate Door to Roof (1) | 8.6 mm (0.34 in) | 0.0 to -1.0 mm (0.00 to -0.04 in)
Liftgate Door to Roof (4) | 5.6 mm (0.22 in) | 0.0 to -1.0 mm (0.00 to -0.04 in)
Liftgate Door to Extension Back Panel (5) | 3.8-5.8 mm (0.15-0.23 in)* | --
Liftgate Door to Rear Combination Lamp (6) | 5.2 mm (0.205 in) | 2.5 mm (0.098 in)
*Difference of the left and the right side: 1.0 mm (0.04 in) maximum

## Body Rear End Adjustment Specifications 4 Door

#### Sheet Metal Tolerances--4-Door Model

Location | Clearance Gap | Flushness
--- | --- | ---
Important: Use the following specifications in order to ensure the proper clearances and flushness of the rear end body components after body repair procedures are complete.
Rear Door to Quarter Panel (1) | 5.1 mm (0.20 in) | 0.0-1.0 mm (0.00-0.04 in)
Trunk Lid to Quarter Panel (2) | 3.6 mm (0.14 in) | -1.8 to 0.0 mm (-0.07 to 0.00 in)
Trunk Lid to Rear Window (5) | 5.0 mm (0.20 in) | -2.6 mm (-0.102 in)
Trunk Lid to Rear Combination Lamp (4) | 0.3 mm (0.012 in) | --
Trunk Lid to Extension Back Panel (3) | 4.2 mm (0.17 in) See Note | -1.0 to 0.0 mm (-0.4 to 0.00 in)
Difference of the left and the right side: 1.0 mm (0.04 in) maximum