For 1990-2009 cars

### Removal Procedure

1. Remove the left side headlamp. Refer to Headlamp Replacement in Lighting Systems.
2. Remove the two bolts from the left inner fender.
3. Drain the hose. Pull the recovery reservoir (1) out of the fender mount.
4. If reusing the original reservoir, clean the inside and the outside of the coolant recovery reservoir and cap (4) with soap and water.

### Installation Procedure

1. Install the coolant recovery reservoir to the left fender with two bolts.
2. Install the recovery reservoir hose.
3. Install the left side headlamp. Refer to Headlamp Replacement in Lighting Systems.