For 1990-2009 cars

### Removal Procedure

1. Disconnect the daytime running lamp (DRL) control module electrical connector (1) .
2. Remove the following components from the vehicle:

2.1. | The mounting screw (3)

2.2. | The DRL control module (2)

### Installation Procedure

1. Install the DRL control module (2) to the vehicle. Secure the module with the mounting screw (3).
2. Connect the DRL electrical connector (1).