For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Control Module | Below the right side of the IP, attached to the evaporator case | HVAC Component Views in HVAC | HVAC Connector End Views in HVAC
Blower Speed Selector Switch | Center of the IP, above the radio | HVAC Component Views in HVAC | --
Camshaft Position Sensor | Cylinder head, near the ignition coil 2 | Engine Controls Component Views | --
Clutch Pedal Position (CPP) Switch (Manual Transaxle) | Mounted above the clutch pedal | Engine Electrical Component Views in Engine Electrical | --
Crankshaft Position Sensor | Bottom of the engine, mounted to the engine, near the crankshaft pulley | Engine Controls Component Views | Engine Controls Connector End Views
Data Link Connector (DLC) OBD 2 | Below the left side of the IP, near the center console | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Diode Module | Behind the center IP, taped to the IP harness | Lighting Systems Component Views in Lighting Systems | Engine Controls Connector End Views
Direct Clutch Solenoid (Automatic Transaxle) | Left rear side of the transaxle, attached to the valve body | -- | --
Duty Check Data Link Connector | Passenger compartment, taped to the harness, behind the IP compartment | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Engine Cooling Fan Motor | Left front side of the engine compartment, behind the radiator | -- | Cooling System Connector End Views in Engine Cooling
EVAP Canister Purge Valve | Center of the engine compartment, on the intake manifold | Engine Controls Component Views | Engine Controls Connector End Views
EVAP Canister Vent Solenoid | Top of the fuel tank | Engine Controls Component Views | Engine Controls Connector End Views
EVAP Tank Pressure Control Solenoid Valve | Top of the fuel tank | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Injector No. 1 | Top of the engine, in the intake port 1 | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Injector No. 2 | Top of the engine, in the intake port 2 | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Injector No. 3 | Top of the engine, in the intake port 3 | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Injector No. 4 | Top of the engine, in the intake port 4 | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Sender Assembly | In the fuel tank | Engine Controls Component Views | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges, and Console
Fuel Tank Pressure Sensor | In the fuel tank | Engine Controls Component Views | Engine Controls Connector End Views
Fuse Box | Left side of the engine compartment, mounted on the left inner side of the fender, behind the relay box | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Heated Oxygen Sensor 1 (HO2S1) | Front of the engine in the exhaust manifold | Engine Controls Component Views | Engine Controls Connector End Views
Heated Oxygen Sensor 2 (HO2S2) | Below the vehicle, behind the three-way catalytic converter (TWC) | Engine Controls Component Views | --
Idle Air Control (IAC) Valve | Top of the engine, mounted to the throttle body | Engine Controls Component Views | Engine Controls Connector End Views
Ignition Coil 1 | On the cylinder head, over spark plug 4 | Engine Controls Component Views | --
Ignition Coil 2 | On the cylinder head, over spark plug 2 | Engine Controls Component Views | --
Ignition Switch | Right side of the steering column | -- | --
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges, and Console
Intake Air Temperature (IAT) Sensor | Center of the engine compartment, attached to the air cleaner housing | Engine Controls Component Views | Engine Controls Connector End Views
Junction Block | Behind the left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Manifold Absolute Pressure (MAP) Sensor | Right rear of the engine compartment, on the bulkhead | Engine Controls Component Views | Engine Controls Connector End Views
Power Steering Pressure Switch | Right front side of the engine compartment, on the power steering pump | Engine Controls Component Views | --
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views | Powertrain Control Module Connector End Views
Rear Defogger Switch | In the IP, to the left of steering column | -- | Stationary Windows Connector End Views in Stationary Windows
Relay Box | Left front of the engine compartment, near the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
2nd Brake Solenoid (Automatic Transaxle) | Left rear side of the transaxle, attached to the valve body | -- | --
Throttle Position (TP) Sensor | Right rear side of the engine, attached to the throttle body | Engine Controls Component Views | Engine Controls Connector End Views
Transaxle Range Switch (Automatic Transaxle) | Left side of the engine compartment, mounted to the top of the transaxle | -- | Automatic Transmission Connector End Views in Transmissions
Turn Signal/Combination Switch | On the steering column | -- | Lighting Systems Connector End Views in Lighting Systems
Vehicle Speed Sensor (VSS) (Automatic Transaxle) | Left side of the engine compartment, on the top of the transaxle | -- | --
C108 (2 Cavities) (Automatic Transaxle) | Engine harness to the transaxle solenoid jumper, on the left rear side of the transaxle | Harness Routing Views in Wiring Systems | --
C112 (16 Cavities) | Main harness to the engine harness, in the right rear side of the engine compartment, near the bulkhead | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C113 (16 Cavities) | Main harness to the engine harness, in the right rear side of the engine compartment, near the bulkhead | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 (14 Cavities) | Main harness to the floor harness, behind the left side of the IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C203 (13 Cavities) | IP harness to the floor harness, behind the left side of the IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C204 (2 Cavities) (Manual Transaxle) | Main harness to the clutch pedal position switch, behind the left side of the IP | Harness Routing Views in Wiring Systems | --
C205 (12 Cavities) | IP harness to the engine harness, behind the right side of the IP, near the powertrain control module (PCM) | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C211 (6 Cavities) | IP harness to the jumper of the blower speed selector switch, behind the center of the IP | Harness Routing Views in Wiring Systems | --
C300 (2 Cavities) | Floor harness to the jumper harness of the fuel tank, under the rear passenger seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C310 (4 Cavities) | Floor harness to the jumper harness of the fuel tank, under the rear passenger seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C311 (3 Cavities) | Floor harness to the jumper harness of the fuel tank, under the rear passenger seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G102 | Left front side of the engine compartment, on the left-front inner fender, near the battery | Harness Routing Views in Wiring Systems | --
G104 | Left end of the cylinder head | Harness Routing Views in Wiring Systems | --
G203 | Junction block case ground, under the left side of the IP | -- | --
G400 (2-Door) | Rear center of the luggage compartment | Harness Routing Views in Wiring Systems | --
(4-Door) | Rear center of the luggage compartment | Harness Routing Views in Wiring Systems | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views in Wiring Systems | --
P202 | Center of the engine compartment, on the bulkhead | Harness Routing Views in Wiring Systems | --
P300 | Below the right rear passenger seat | Harness Routing Views in Wiring Systems | --
S101 | Main harness, approximately 11 cm (4.5 in) from the breakout of the brake fluid level switch | Harness Routing Views in Wiring Systems | --
S111 | Main harness, approximately 7 cm (2.8 in) from the ignition coil breakout | -- | --
S119 | Main harness, approximately 50 cm (20 in) from the connector breakout of the front wiper motor | Harness Routing Views in Wiring Systems | --
S126 | Engine harness, approximately 8 cm (3.1 in) from P202 | Harness Routing Views in Wiring Systems | --
S127 (Manual Transaxle) | Engine harness, at the generator breakout | -- | --
(Automatic Transaxle) | Engine harness, 5 cm (2 in) from the starter breakout | -- | --
S129 | Engine harness, approximately 2 cm (1 in) from the C113 breakout | -- | --
S130 | Engine harness, approximately 5 cm (2 in) from the starter breakout | Harness Routing Views in Wiring Systems | --
S131 | Engine harness, approximately 9 cm (3.6 in) from the connector breakout of the generator | Harness Routing Views in Wiring Systems | --
S151 | Main harness, approximately 5 cm (2 in) from the relay box | Harness Routing Views in Wiring Systems | --
S152 | Main harness, approximately 19 cm (7.4 in) from the C113 breakout | Harness Routing Views in Wiring Systems | --
S153 | Main harness, approximately 13 cm (5.125 in) from the connector breakout of the front wiper motor | Harness Routing Views in Wiring Systems | --
S154 (Automatic Transaxle) | Engine Harness, approximately 9 cm (3.6 in) from P202 | Harness Routing Views in Wiring Systems | --
S156 | Engine harness, approximately 7 cm (3 in) from P202 | Harness Routing Views in Wiring Systems | --
S158 (Automatic Transaxle) | Engine harness, approximately 19 cm (1.5 in) from P202 | -- | --
S159 | Engine Harness, approximately 2 cm (1 in) from C113 | Harness Routing Views in Wiring Systems | --
S160 | Engine Harness, approximately 20 cm (8 in) from P202 | -- | --
S161 | Engine harness, approximately 4 cm (2 in) from the generator breakout | -- | --
S163 | Engine harness, approximately 2 cm (1 in) from the fuel injectors breakout | -- | --
S164 | Engine harness, approximately 8 cm (3.125 in) from the breakout of the MAP sensor | Harness Routing Views in Wiring Systems | --
S165 | Engine harness, approximately 5 cm (2 in) from the starter breakout | Harness Routing Views in Wiring Systems | --
S166 | Engine harness, approximately 7 cm ( in) from the breakout of fuel injector No. 1 | -- | --
S167 | Engine harness, approximately 14 cm (6 in) from the C113 breakout | Harness Routing Views in Wiring Systems | --
S202 | Main harness, approximately 8 cm (3.125 in) from the breakout of the junction block connector C6 | -- | --
S204 | Main harness, approximately 8 cm (3.125 in) from the breakout of junction-block connector C5 | -- | --
S208 (With ABS) | Main harness, approximately 12 (5 in) cm from the G201 breakout | -- | --
S218 | IP harness, approximately 3 cm (1.19 in) from the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S221 | IP harness, approximately 7 cm (3 in) from the breakout of IP cluster assembly connector C2 | Harness Routing Views in Wiring Systems | --
S222 | IP harness, approximately 6 cm (2.375 in) from the breakout of the data link connector | Harness Routing Views in Wiring Systems | --
S225 | IP harness, approximately 2 cm (1 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S226 | IP harness, approximately 3 cm (1.19 in) from the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S231 | Main harness, approximately 15 (6 in) cm from P200 | -- | --
S233 | IP harness, approximately 8 cm (3.125 in) from the blower motor branch breakout | Harness Routing Views in Wiring Systems | --
S234 | IP harness, approximately 1 cm (0.375 in) from the breakout of the diode module connector | Harness Routing Views in Wiring Systems | --
S235 | IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views in Wiring Systems | --
S236 | IP harness, approximately 8 cm (3.125 in) from the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S237 | IP harness, approximately 10 cm (4 in) from the breakout of the radio connector | Harness Routing Views in Wiring Systems | --
S240 | IP harness, approximately 6 cm (2.375 in) from the breakout of the data link connector | Harness Routing Views in Wiring Systems | --
S241 | IP harness, approximately 5 cm (2 in) from the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S242 | IP harness, at the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S245 | IP harness, approximately 12 cm (5 in) from the breakout of IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S248 | Engine harness, approximately 4 cm (2 in) from the breakout of powertrain control module (PCM) connector C1 | Harness Routing Views in Wiring Systems | --
S251 (With ABS) | Main harness, approximately 5 cm (2 in) from P200 | -- | --
S252 | IP harness, approximately 4 cm (2 in) from the breakout of the data link connector | Harness Routing Views in Wiring Systems | --
S256 | Main harness, near the breakout of connector C6 of the junction block | -- | --
S259 | Engine harness, approximately 6 cm (2.375 in) from P202 | Harness Routing Views in Wiring Systems | --
S261 (Manual Transaxle) | Engine harness, approximately 4 cm (2 in) from the breakout of the PCM connectors | Harness Routing Views in Wiring Systems | --
S262 | Engine harness, approximately 5 cm (2 in) from P202 | Harness Routing Views in Wiring Systems | --
S263 | Engine harness, approximately 3 cm (1.9 in) from the C205 breakout | Harness Routing Views in Wiring Systems | --
S301 (2-Door) | Floor harness, approximately 20 cm (8 in) from the center console branch breakout | Harness Routing Views in Wiring Systems | --
S311 (4-Door) | Floor harness, approximately 10 cm (4 in) from the C400 breakout | Harness Routing Views in Wiring Systems | --
S315 | Jumper harness of the fuel tank, approximately 10 cm (4 in) from P300 | Harness Routing Views in Wiring Systems | --
S316 | Jumper harness of the fuel tank, approximately 20 cm (8 in) from P300 | Harness Routing Views in Wiring Systems | --