For 1990-2009 cars

The EBCM contains sophisticated on-board diagnostics. When a Scan Tool accesses the EBCM on-board diagnostics, the EBCM on-board diagnostics identify the source of any system malfunction as specifically as possible. The EBCM on-board diagnostics also diagnose whether the malfunction is intermittent.

The following actions occur when using the Scan Tool with ABS:

• | The Scan Tool specifically identifies the last DTC.

• | The specific ABS data stores at the time of the malfunction.

• | Information about the first five DTCs set and the last DTC set becomes available.

• | The input and output can be monitored.

• | Malfunction confirmation and repair verification are enabled.

• | The manual control of components and the automated functional tests become available.