For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Was the Charging System Check performed? | -- | Go to Step 2 | Go to Charging System Check
2 |

1. Disconnect the generator connector.
2. Turn the ignition switch to ON.

Does the charge indicator light?

--

Go to Step 4

Go to Step 3

3 | Repair or replace the generator. Refer to Generator Replacement and Generator Overhaul . Is the repair complete? | -- | Go to Charging System Check | --
4 |

1. Turn the ignition switch to LOCK.
2. Disconnect the DRL control module connector.
3. Turn the ignition switch to ON.

Does the charge indicator light?

--

Go to Step 6

Go to Step 5

5 | Replace the DRL control module. Is the repair complete? | -- | Go to Charging System Check | --
6 | Test for a short to ground in the WHT/RED wire between the instrument panel cluster and the generator. Was a short found? | -- | Go to Step 7 | Go to Step 8
7 | Repair the short. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Charging System Check | --
8 | Repair or replace the instrument cluster printed circuit. Is the repair complete? | -- | Go to Charging System Check | --