For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Was the Interior Lights System Check performed? | -- | Go to Step 2 | Go to Interior Lamps System Check
2 | Backprobe the luggage compartment lamp connector with a test light from cavity 1 to ground. Does the test lamp light? | -- | Go to Step 3 | Go to Step 5
3 | Test for an open in the BLK/YEL wire between the luggage compartment lamp and the luggage compartment lamp switch. Was an open found? | -- | Go to Step 7 | Go to Step 4
4 | Replace the luggage-compartment lamp switch. Refer to Liftgate Lock System Replacement (2-Door) or Lock System Replacement - Rear Compartment (4-Door) in Body Rear End. Is the repair complete? | -- | Go to Interior Lamps System Check | --
5 | Test for an open in the WHT wire between the junction block and the luggage compartment lamp. Was an open found? | -- | Go to Step 7 | Go to Step 6
6 | Replace the junction block. Is the repair complete? | -- | Go to Interior Lamps System Check | --
7 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lamps System Check | --