For 1990-2009 cars

### Removal Procedure

1. Remove the wheelhousing (2) from the front fender fascia by removing 1 screw and 3 plastic retaining clips (5).
2. Remove the wheelhousing (2) from the front fender (1) by removing the 5 screws (4,6).

### Installation Procedure

1. Install the wheelhousing (2) to the fender (1). Secure the wheelhousing with 5 screws (4,6).
2. Install the wheelhousing (2) to the front fender fascia. Secure the wheelhousing with the following components:

• | 1 screw

• | 3 plastic retaining clips (5)