For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Control Module | Below right side of the IP, attached to evaporator case | HVAC Component Views | HVAC Connector End Views
A/C Condenser Fan Motor | Right side of grille, front of A/C condenser | HVAC Component Views | --
A/C Refrigerant (Dual) Pressure Switch | Right rear side of the engine compartment, near the strut tower | -- | --
A/C Switch | Center of IP, above radio | -- | HVAC Connector End Views
Audio Alarm Module | Left side of the lower IP, left of Steering column | Audible Warnings Component Views | Audible Warnings Connector End Views
Backup Lamp Switch (Manual Transaxle) | Left side of the engine compartment, top of transaxle | Lighting Systems Component Views | Lighting Systems Connector End Views
Battery | Left side of engine compartment | Power and Grounding Component Views | --
Blower Motor | Behind the right side of the IP | Heater Blower Controls Component Views | Heater Blower Controls Connector End Views
Blower Speed Selector Switch | Center of IP, above radio | Heater Blower Controls Component Views | --
Brake Fluid Level Switch | In the brake fluid reservoir | -- | Hydraulic Brakes Connector End Views
Camshaft Position Sensor (VIN 2) | Cylinder head, near the ignition coil 2 | Engine Controls Component Views | --
Center High-Mounted Stoplamp (CHMSL) | Bottom of rear window | -- | Lighting Systems Connector End Views
Cigar Lighter | Center of IP, below radio | -- | Power and Grounding Connector End Views
Clutch Pedal Position (CPP) Switch (Manual Transaxle) | Mounted above the clutch pedal | Engine Electrical Component Views | --
Data Link Connector (DLC) OBD 2 | Below the left side of the IP, near the center console | Data Link Communications Component Views | Data Link Communications Connector End Views
Daytime Running Lamps (DRL) Control Module | Behind the left side of the IP | Lighting Systems Component Views | Lighting Systems Connector End Views
Duty Check Data Link Connector | Passenger compartment, taped to the harness behind the IP compartment | Data Link Communications Component Views | Data Link Communications Connector End Views
Early Fuel Evaporation (EFE) Heater (VIN 6) | Mounted between the intake manifold and the throttle body | Engine Controls Component Views | --
Electronic Brake Control Module (EBCM) (With ABS) | Behind the left IP, above the junction block | Antilock Brake System Component Views | Antilock Brakes System Connector End Views
Engine Cooling Fan Motor | Left front side of the engine compartment, behind the radiator | -- | Cooling System Connector End Views
Front Washer Pump | Left front side of the engine compartment, under the washer fluid reservoir | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Front Wiper Motor | Right rear side of the engine compartment, against the bulkhead | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Fuel Sender Assembly | In the fuel tank | Engine Controls Component Views | Instrument Panel, Gages, and Console Connector End Views
Fuse Box | Left side of the engine compartment, mounted on Left inner side of the fender, behind the relay box | Power and Grounding Component Views | Power and Grounding Connector End Views
Generator | Right rear side of the engine compartment, mounted to the engine | Engine Electrical Component Views | --
Heated Oxygen Sensor 1 (HO2S1) | Front of the engine in the exhaust manifold | Engine Controls Component Views | Engine Controls Connector End Views
Heated Oxygen Sensor 2 (HO2S2) | Below vehicle after a three-way catalytic converter (TWC) | Engine Controls Component Views | --
Horn | Left front side of the engine compartment, behind the grille | Horn Component Views | --
Idle Air Control (IAC) Valve (VIN 2) | Top of engine, mounted to the throttle body | Engine Controls Component Views | Engine Controls Connector End Views
Idle Speed Control (ISC) Motor (VIN 6) | Top of engine, mounted to the throttle body | Engine Controls Component Views | --
Ignition Control Module (VIN 6) | Left engine compartment on the bulkhead near the strut tower | Engine Controls Component Views | --
Ignition Coil (VIN 6) | Left side of the engine compartment, on the bulkhead | Engine Controls Component Views | --
Ignition Coil 1 (VIN 2) | On the cylinder head, over spark plug 4 | Engine Controls Component Views | --
Ignition Coil 2 (VIN 2) | On the cylinder head, over spark plug 2 | Engine Controls Component Views | --
Ignition Key Warning Switch | Right side of the steering column, on the ignition switch cylinder | -- | --
Ignition Switch | Right side of the steering column | -- | --
Illumination Controller | In the IP, left of the steering column | -- | Lighting Systems Connector End Views
Inflatable Restraint Forward Discriminating Sensor | Front center of the grille, behind the hood latch assembly | SIR Component Views | --
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Center of the console, in front of the manual selector | SIR Component Views | SIR Connector End Views
Instrument Panel Cluster Assembly | Left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
Lamp Driver Relay (With ABS) | Behind the left side of the IP, left of the steering column, near electronic brake control module (EBCM) | Antilock Brake System Component Views | Antilock Brakes System Connector End Views
LH Power Door Lock Switch (4-Door With Power Door Locks) | Left front door trim panel | Power Door Systems Component Views | Power Door Systems Connector End Views
Luggage Compartment Lamp (4-Door) | Center of the luggage compartment, under rear window shelf | Lighting Systems Component Views | Lighting Systems Connector End Views
Noise Suppressor Filter (VIN 6) | Left rear engine compartment, taped to the harness, below the ignition control module | Engine Controls Component Views | --
Power Door Lock Control Module (4-Door with Power Door Locks) | Left side of the IP, mounted to A-pillar, above the left kick panel | Power Door Systems Component Views | Power Door Systems Connector End Views
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views | Powertrain Control Module Connector End Views in Engine Controls - 1.3L or Powertrain Control Module Connector End Views in Engine Controls - 1.0L.
Radio | Center of the IP | -- | Entertainment Connector End Views
Rear Defogger | In the rear window | Stationary Windows Component Views | --
Rear Defogger Switch | In the IP, left of steering column | -- | Stationary Windows Connector End Views
Rear Washer Pump (2-Door LSi) | Left front side of the engine compartment under washer fluid reservoir | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Rear Wiper Motor (2-Door LSi) | Center of the liftgate | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Rear Wiper/Washer Switch (2-Door LSi) | In IP, left of the steering column | -- | Wiper/Washer Connector End Views
Relay Box | Left front engine compartment, near the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
RH Power Door Lock Switch (4-Door With Power Door Locks) | In the right front door trim panel | Power Door Systems Component Views | Power Door Systems Connector End Views
Seat Belt Switch | In left seat belt buckle | -- | Audible Warnings Connector End Views
Shift Lock Solenoid (Automatic Transaxle) | Near base of manual selector | -- | --
Starter Solenoid | Center rear of engine, top of the starter motor | Engine Electrical Component Views | --
Stoplamp Switch | Top of brake pedal | Lighting Systems Component Views | Lighting Systems Connector End Views
Supplemental Inflator Restraint Data Link Connector (SIR DLC) | Behind the left lP near the junction block | -- | Data Link Communications Connector End Views
Transaxle Range Switch (Automatic Transaxle) | Left side of the engine compartment, mounted to top of the transaxle | -- | Automatic Transmission Connector End Views
Turn Signal/Combination Switch | On steering column | -- | Lighting Systems Connector End Views
C112 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near bulkhead | Harness Routing Views | Inline Harness Connector End Views
C113 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near the bulkhead | Harness Routing Views | Inline Harness Connector End Views
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C204 (2 Cavities) (Manual Transaxle) | Main harness to clutch pedal position switch, behind left side of the IP | Harness Routing Views | --
C207 (3 Cavities) | IP harness to dome lamp harness, right side of the upper cowl | Harness Routing Views | Inline Harness Connector End Views
C208 (8 Cavities) | Main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views | Inline Harness Connector End Views
C210 (5 Cavities) | Supplemental inflatable restraint (SIR) harness to the IP harness, behind the left side of the IP, near the junction block | Harness Routing Views | Inline Harness Connector End Views
C211 (6 Cavities) | IP harness to blower speed selector switch jumper, behind the center of the IP | Harness Routing Views | --
C212 (6 Cavities) (4-Door) | Floor harness to left front door, behind the left kick panel | Harness Routing Views | Inline Harness Connector End Views
C213 (6 Cavities) (4-Door) | Floor harness to right front door, behind right kick panel | Harness Routing Views | Inline Harness Connector End Views
C300 (2 Cavities) | Floor harness to fuel tank jumper harness, under the rear passenger seat | Harness Routing Views | Inline Harness Connector End Views
C311 (3 Cavities) | Floor harness to fuel tank jumper harness, under the rear passenger seat | Harness Routing Views | Inline Harness Connector End Views
C400 (10 Cavities) (4-Door) | Floor harness to luggage compartment harness, left front side of luggage compartment near the left rear speaker | Harness Routing Views | --
C402 (6 Cavities) (2-Door) | Floor harness to liftgate harness, right rear corner of vehicle | Harness Routing Views | --
G100 | Mounted on top of the left side of the transaxle | -- | --
G101 | Left front side of the engine compartment, front of the battery | -- | --
G102 | Left front side of the engine compartment on the left front inner fender near battery | Harness Routing Views | --
G103 | Right front side of the engine compartment on the right front side of the inner fender | Harness Routing Views | --
G104 | Center rear side of the engine on the intake manifold | Harness Routing Views | --
G105 (VIN 6) | Center rear of engine, on the intake manifold | -- | --
G201 | Behind the left side of the kick panel | Harness Routing Views | --
G202 | Right side of the center IP behind the radio | Harness Routing Views | --
G203 | Junction block case ground, under the left side of the IP | -- | --
G204 | Behind right side of the kick panel | -- | --
G300 (4-Door) | Behind the right rear quarter trim panel | -- | --
G400 | Rear center of luggage compartment | -- | --
G401 (2-Door) | Center of the liftgate, near rear wiper motor | Harness Routing Views | --
G402 (2-Door) | Left side of the liftgate behind trim panel | -- | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views | --
P202 | Center of the engine compartment, on the bulkhead | Harness Routing Views | --
P203 | Behind the right kick panel | -- | --
P300 | Below the right rear passenger seat | Harness Routing Views | --
P400 | Left rear side of the luggage compartment | -- | --
P401 | Right rear of luggage compartment | -- | --
P402 | Center rear side of the luggage compartment | Harness Routing Views | --
P403 (2-Door) | Upper right side of the liftgate | Harness Routing Views | --
P500 | Left front door | -- | --
P600 | Right front door | -- | --
S101 | Main harness, approximately 11 cm (4.5 in) from the brake fluid level switch breakout | Harness Routing Views | --
S111 (VIN 6) | Main harness, approximately 7 cm (2.8 in) from the ignition coil breakout | -- | --
S117 | Main harness, at the G103 breakout | Harness Routing Views | --
S122 | Main harness, at relay box | Harness Routing Views | --
S126 | Engine harness, approximately 8 cm (3.1 in) from P202 | Harness Routing Views | --
S130 | Engine harness, approximately 5 cm (2 in) from starter breakout | Harness Routing Views | --
S134 | A/C jumper harness, approximately 15 cm (6 in) from the G103 breakout | -- | --
S151 | Main harness, approximately 5 cm (2 in) from the relay box | Harness Routing Views | --
S152 | Main harness, approximately 19 cm (7.4 in) from the C113 breakout | Harness Routing Views | --
S160 (VIN 2) | Engine Harness, approximately 20 cm (8 in) from P202 | -- | --
S161 (VIN 2) | Engine harness, approximately 4 cm (2 in) from the generator breakout | -- | --
S165 (VIN 2) | Engine harness, approximately 5 cm (2 in) from the starter breakout | Harness Routing Views | --
S167 | Engine harness, approximately 14 cm (6 in) from the C113 breakout | Harness Routing Views | --
S202 | Main harness, approximately 8 cm (3.125 in) from the junction block connector C6 breakout | -- | --
S207 | Main harness, approximately 12 cm (5 in) from the G201 breakout | -- | --
S208 (With ABS) | Main harness, approximately 12 (5 in) cm from the G201 breakout | -- | --
S209 | Main harness, approximately 2 cm (1 in) from the G201 breakout | -- | --
S210 | Main harness, approximately 15 cm (6 in) from C208 | -- | --
S213 | Main harness, approximately 8 cm (3.125 in) from P200 | -- | --
S215 (With ABS) | Main harness, approximately 4 cm (2 in) from the junction block connector C6 breakout | -- | --
S222 | IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC-OBD2) breakout | Harness Routing Views | --
S224 | IP harness, approximately 5 cm (2 in) from data link connector - (DLC-OBD2) breakout | Harness Routing Views | --
S235 | IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views | --
S236 | IP harness, approximately 8 cm (3.125 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S237 | IP harness, approximately 10 cm (4 in) from the radio connector breakout | Harness Routing Views | --
S238 | IP harness, approximately 3 cm (1.19 in) from the blower motor connector breakout | Harness Routing Views | --
S239 | IP harness, approximately 11 cm (4.313 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S240 | IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC-OBD2) breakout | Harness Routing Views | --
S241 | IP harness, approximately 5 cm (2 in) from the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S242 | IP harness, at the IP cluster assembly connector C3 breakout | Harness Routing Views | --
S243 | IP harness, approximately 5 cm (2 in) from the cigar lighter connector breakout | Harness Routing Views | --
S244 | Main harness, approximately 23 cm (9.06 in) from P200 | -- | --
S245 | IP harness, approximately 12 cm (5 in) from the I/P cluster assembly connector C3 breakout | Harness Routing Views | --
S247 | Main harness, approximately 18 cm (7.06 in) from P200 | -- | --
S254 | IP harness, approximately 6 cm (2.375 in) from the C215 breakout | Harness Routing Views | --
S256 | Main harness, near the junction block connector C6 breakout |  | --
S263 | Engine harness, approximately 3 cm (1.9 in) from the C205 breakout | Harness Routing Views | --
S301 (2-Door) | Floor harness, approximately 20 cm (8 in) from the center console branch breakout | Harness Routing Views | --
S314 (4-Door With Power Door Locks) | Floor harness, approximately 25 cm (10 in) from the C201 breakout | Harness Routing Views | --
S315 | Fuel tank jumper harness, approximately 10 cm (4 in) from P300 | Harness Routing Views | --
S402 (2-Door) | Floor harness, approximately 5 cm (2 in) from the left rear combination lamp connector breakout | -- | --
S403 (2-Door) | Floor Harness, approximately 5 cm (2 in) from G400 breakout | -- | --
S406 (4-Door) | Floor harness, approximately 10 cm (4 in) from the left rear combination lamp connector breakout | -- | --
S407 (4-Door) | Floor harness, approximately 20 cm (8 in)from the left rear combination lamp connector breakout | -- | --
S408 (4-Door) | Floor harness, approximately 5 cm (2 in) from the C400 breakout | -- | --