For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws (1, 7) from the headlamp (6).
2. Turn the park and turn lamp bulb socket (8) counterclockwise in order to remove the socket from the headlamp (6).
3. Remove the park and turn lamp bulb (8) from the socket, if necessary.

### Installation Procedure

1. Install the park and turn lamp bulb (8) to the park and turn lamp bulb socket, if removed.
2. Rotate the park and turn lamp bulb socket (8) clockwise in order to secure the socket to the headlamp (6).
3. Install the headlamp (6) to the vehicle. Secure the headlamp with the 2 screws (1, 7).
4. Adjust the headlamp aim. Refer to Headlamp Aiming .