For 1990-2009 cars

### Removal Procedure

1. Remove the center pillar lower trim panel (10) from the vehicle by gently prying the panel loose.
2. Loosen the door opening lace on both sides of the center pillar upper trim panel.
3. Remove the plastic retainer and the center pillar upper trim panel (5) from the vehicle.

### Installation Procedure

1. Install the center pillar upper trim panel (5) to the vehicle. Secure the trim panel with the plastic retainer.
2. Press the door opening lace into place on both sides of the trim panel.
3. Install the center pillar lower trim panel (10) to the vehicle