For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Battery Carrier Retaining Bolts | 15 N·m | 11 lb ft
Battery Hold-Down Bracket Retaining Bolt | 15 N·m | 11 lb ft
Fender Brace-to-Vehicle Retaining Bolt | 20 N·m | 15 lb ft
Fender-to-Bumper Fascia Support Nut | 20 N·m | 15 lb ft
Fender Retaining Bolts | 20 N·m | 15 lb ft
Hood Hinge Retaining Bolts | 27 N·m | 20 lb ft
Hood Latch Retaining Bolts | 7 N·m | 62 lb in
Hood Retaining Bolts | 27 N·m | 20 lb ft
Wiper Arm Retaining Nut | 20 N·m | 15 lb ft