For 1990-2009 cars

### Removal Procedure

1. Remove the rear seat back cover. Refer to Rear Seat Back Cushion Cover and Pad Replacement .
2. Remove the following components from the vehicle:

2.1. | 2 bolts (2)

2.2. | The seat back lock (1)

### Installation Procedure

1. Install the seat back lock (1) to the seat back. Secure the lock with 2 bolts (2).
2. Install the rear seat back cover. Refer to Rear Seat Back Cushion Cover and Pad Replacement .