For 1990-2009 cars

### Removal Procedure

1. Disconnect the antenna connector from the back of the radio. Access through the instrument panel compartment.
2. Remove the antenna cable from the clips under the instrument panel.
3. Remove 2 clips and the left hinge pillar trim panel from the vehicle.
4. Remove the left windshield side garnish molding.
5. Remove the antenna cable from the clips on the left windshield side panel.
6. Attach a piece of rigid wire (1) to the antenna cable (2). This will aid in the removal and the installation of the cable through the windshield side pillar.
7. Remove the following components from the roof of the vehicle:

7.1. | 2 antenna mast screws

7.2. | The antenna mast (1)

8. Remove the rigid wire (1) from the antenna cable (2). Leave the rigid wire in the windshield in order to aid in antenna installation.

### Installation Procedure

1. Attach the rigid wire (1) to the antenna cable (2).
2. Guide the antenna cable and the antenna mast (1) through the windshield side pillar with the aid of the rigid wire.
3. Install the antenna mast screws.
4. Remove the rigid wire (1) from the antenna cable (2).
5. Install the antenna cable to the clips on the left windshield side panel.
6. Install the left windshield side garnish molding.
7. Install the left hinge pillar trim panel to the vehicle. Secure the trim panel with the 2 clips.
8. Install the antenna cable to the clips under the instrument panel.
9. Connect the antenna connector to the radio. Access through the instrument panel compartment.