For 1990-2009 cars

### Removal Procedure

1. Remove the 3 screws (2) and the rear door front molding (1) from the rear door.
2. Remove the rear door rear molding. Refer to Rear Side Door Window Reveal Molding Replacement .
3. Partially lower the door window weather strip (1) in order to gain the necessary clearance to remove the door opening weather strip (3).
4. Remove the 2 plastic retainers that retain the rear door opening molding (1).
5. Pull the molding (1) from the door (2).

### Installation Procedure

1. Install the door opening weather strip (1) to the rear door. Secure the molding with the 2 plastic retainers.
2. Install the door window weather strip (1) to the door (2).
3. Install the rear door rear molding. Refer to Rear Side Door Window Reveal Molding Replacement .
4. Install the rear door front molding (1) to the door. Secure the molding with the 3 screws (2).