For 1990-2009 cars

### Removal Procedure

1. For vehicles equipped with a manual transaxle, remove the gearshift control lever upper boot (2) from the console (3).
2. Remove the console (3) from the vehicle by removing 6 screws.

### Installation Procedure

1. Install the console (3) to the vehicle. Secure the console with the 6 screws.
2. For vehicles equipped with a manual transaxle, install the gearshift control lever upper boot (2) to the console (3).