For 1990-2009 cars

1. Remove the 8 bolts and the 1 nut which secure the timing belt cover.
2. Remove the timing belt cover (12).

Important: Before removing the timing belt, align the upper timing marks and the lower timing marks by turning the crankshaft.

3. Ensure that the upper timing marks (1, 2) are aligned.
4. Ensure that the lower timing marks (1, 2) are aligned.
5. Loosen the timing belt tensioner bolt (2) and the stud (1).
6. Push up the tensioner plate completely with your finger.Remove the belt from the crankshaft timing belt pulley and from the camshaft timing belt pulley.
7. Inspect the timing belt for wear or for cracks. Replace the timing belt as necessary.