For 1990-2009 cars

#### Tools Required

• | J 24086-C Piston Pin Remover/Installer

• | J 24086-150 Fork Insert

• | J 24086-900 Universal Fork

Caution: Wear safety glasses in order to avoid eye damage.

1. Remove the piston rings from the pistons. Use a suitable tool in order to expand the rings.
2. Mark, separate, and organize the rings for assembly.
3. Press the piston pin from the connecting rod using the J 24086-C .

The piston pin has an interference fit into the connecting rod, and is full floating in the piston.

4. Mark, separate, and organize the parts for assembly.