For 1990-2009 cars

## Tail Lamp Bulb Replacement 2 Door

### Removal Procedure

1. Remove the 2 screws which secure the tail lamp (5).
2. Pull the tail lamp (5) upward and rearward in order to remove the lamp from the vehicle.
3. Remove the tail lamp bulb socket from the tail lamp (5).
4. Remove the tail lamp bulb (3) from the socket.

### Installation Procedure

1. Install the tail lamp bulb (3) to the tail lamp bulb socket.
2. Install the tail lamp bulb socket to the tail lamp (5).
3. Install the tail lamp (5) to the body. Secure the lamp with the 2 screws.

## Tail Lamp Bulb Replacement 4 Door

### Removal Procedure

1. Open the rear-compartment lid.
2. Reposition the rear compartment side trim in order to access the nut that retains the tail lamp.
3. Remove the nut that retains the tail lamp (1).
4. Remove the 2 screws that retain the tail lamp (1).
5. Remove the tail lamp (1) from the body in order to access the tail lamp bulb socket.
6. Remove the tail lamp bulb socket from the tail lamp (1).
7. Remove the tail lamp bulb (3) from the socket.

### Installation Procedure

1. Install the tail lamp bulb (3) to the tail lamp bulb socket.
2. Install the socket to the tail lamp (1).
3. Install the tail lamp (1) to the vehicle. Secure the lamp with the 2 screws and with the nut.
4. Position the rear compartment side trim back to the original position.
5. Close the rear-compartment lid.