For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Pedal Travel | 60 mm | 2.36 in
Brake Pipe-to-Moving Parts Distance | 19 mm | 0.75 in
Clearance Between the Master Cylinder Piston and the Booster Piston Rod Adjusting Nut | 0 mm | 0 in
Push Rod Clevis Length | 99.5-100.5 mm | 3.92-3.96 in
Stoplamp Switch-to-Brake Pedal Contact Plate Distance | 1.5-2.0 mm | 0.06-0.08 in