For 1990-2009 cars

### Removal Procedure

#### Tools Required

J 28712 Drive Axle Boot Protectors

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle in General Information.
2. Place a drain pan or a suitable container under the transaxle fluid pan.
3. Remove the transaxle drain plug (1) from the transaxle fluid pan (3), and drain the fluid fluid.
4. Install J 28712 to the wheel-side joints of the drive axle and to the differential-side joints of the drive axle.
5. Remove the drive axle assembly from the vehicle. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
6. Remove the fluid seal from the transaxle.
7. Inspect the differential-side joint surface where the drive axle makes contact with the fluid seal of the drive axle shaft.

The surface should be smooth and free of any damage.

If damage to the differential-side joint is evident, replace the differential-side joint.

### Installation Procedure

#### Tools Required

• | J 35538 Axle Shaft Seal Installer

• | J 28712 Drive Axle Boot Protector

1. Install the new seal into the transaxle using the J 35538 .
2. Install the drive axle assembly into the vehicle. Refer to Wheel Drive Shaft Replacement in Wheel Drive Shafts.
3. Remove the J 28712 from the wheel-side joints of the drive axle and from the differential-side joints of the drive axle.
4. Apply GM P/N 12346004, or the equivalent, to the threaded portion of the transaxle drain plug.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

5. Install the transaxle drain plug into the transaxle fluid pan.

Tighten
Tighten the transaxle drain plug to 23 N·m (17 lb ft).

6. Lower the vehicle.
7. Refill the transaxle, as necessary. Refer to Transmission Fluid Check .