For 1990-2009 cars

## Rear Side Marker Lamp Replacement 2-Door

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the 2 screws which secure the tail lamp (5).
3. Pull the tail lamp (5) away from the rear end panel in order to gain access to the socket of the marker lamp bulb.
4. Remove the marker lamp socket from the tail lamp (5).
5. Remove the marker lamp bulb (4) from the socket.

### Installation Procedure

1. Install the marker lamp bulb (4) to the marker lamp socket.
2. Install the marker lamp socket to the tail lamp (5).
3. Install the tail lamp (5) to the rear end panel. Secure the lamp with the 2 screws
4. Connect the negative battery cable.