For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Bearing Set Shim Clearance | 0.08-0.12 mm | 0.0032-0.0047 in
Fifth Speed Locating Spring Standard Length | 26.1 mm | 1.028 in
Fifth Speed Locating Spring Service Limit | 25.0 mm | 0.984 in
High Speed Gearshift Fork-to-High Speed Synchronizer Sleeve Clearance (Maximum) | 1.0 mm | 0.039 in
High Speed Locating Spring Standard Length | 40.1 mm | 1.597 in
High Speed Locating Spring Service Limit | 39.0 mm | 1.535 in
Left Differential Side Gear End Play (Standard) | 0.05-0.33 mm | 0.002-0.013 in
Left Differential Side Gear End Play (Maximum) | 0.05 mm | 0.002 in
Low Speed Gearshift Fork-to-Low Speed Synchronizer Sleeve Clearance (Maximum) | 1.0 mm | 0.039 in
Reverse Gearshift Lever to Idler Shaft Clearance | 5 mm | 0.20 in
Low Speed Locating Spring Standard Length | 26.1 mm | 1.028 in
Low Speed Locating Spring Service Limit | 25.0 mm | 0.984 in
Right Differential Side Gear End Play (Standard) | 0.05-0.33 mm | 0.002-0.013 in
Right Differential Side Gear End Play (Maximum) | 0.05 mm | 0.002 in
Synchronizer Ring-to-Gear Clearance (Standard) | 1.0-1.4 mm | 0.039-0.055 in
Synchronizer Ring-to-Gear Clearance (Minimum) | 1.0-1.4 mm | 0.039-0.055 in

Shim Part Number | Available Shim Thickness
--- | ---
Metric | English
96051167 | 0.8 mm | 0.03 in
96051165 | 1.0 mm | 0.04 in
96051356 | 1.2 mm | 0.05 in
96053031 | 1.4 mm | 0.06 in