For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Disconnect the daytime running lamp (DRL) control module electrical connector (1).
3. Remove the following components from the vehicle:

3.1. | The mounting screw (3)

3.2. | The DRL control module (2)

### Installation Procedure

1. Install the DRL control module (2) to the vehicle. Secure the module with the mounting screw (3).
2. Connect the DRL electrical connector (1).
3. Connect the negative battery cable.