For 1990-2009 cars

### Removal Procedure

1. Remove the air cleaner. Refer to Air Cleaner Assembly Replacement .
2. Disconnect the throttle position (TP) sensor electrical connector.
3. Remove the two screws and the TP sensor.

### Installation Procedure

1. Install the TP sensor to the TBI unit with the two screws, but do not tighten fully.
2. Connect the TP sensor electrical connector.
3. Adjust the TP sensor. Refer to Throttle Position Sensor Adjustment .