For 1990-2009 cars

1. Before installing the new cylinder head gasket, ensure the the oil check valve (3) is properly installed into the cylinder block (2).
2. Install the cylinder head gasket (1).

Install the new cylinder head gasket with the TOP mark facing up (toward the cylinder head) and on the crankshaft timing pulley side.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the cylinder head.

Use the following procedure in order to secure the cylinder head:

3.1. | Apply engine oil to each of the eight cylinder head bolts.

3.2. | Install the eight cylinder head bolts in order to secure the cylinder head.

Install the eight bolts in the order specified in the graphic. Tighten the bolts evenly and in small increments of torque. Repeat the tightening sequence three or four times in order to reach the specified torque.

Tighten
Tighten the cylinder head-to-engine block bolts to 73 N·m (54 lb ft).