For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the System Check? | -- | Go to Step 2 | Go to Radio/Audio System Check
2 |

1. Inspect the moving parts.
2. Inspect the tape head.
3. Use a cleaning cassette in order to clean the moving parts in the cassette player.

Is the cleaning procedure complete?

--

Go to Step 3

--

3 | Use the Diagnostic Test Tape J 39916-A in order to perform the motor speed test. Is the motor speed correct? | -- | Go to Step 5 | Go to Step 4
4 | Replace the radio. Refer to Radio Replacement . Is the repair complete? | -- | Go to Radio/Audio System Check | --
5 | Advise the customer to clean the cassette player periodically. Did you advise the customer? | -- | Go to Radio/Audio System Check | --