For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Audible Warnings System Check? | -- | Go to Step 2 | Go to Audible Warnings System Check
2 |

1. Turn the ignition switch to the LOCK position.
2. Open the LH front door.
3. Disconnect the audio alarm module connector.
4. Connect a J 35616-200 from the audio alarm module connector cavity 6 to B+.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Connect a J 35616-200 from the audio alarm module connector cavity 5 to ground. Does the test lamp light? | -- | Go to Step 5 | Go to Step 6
4 | Use a J 35616-200 in order to backprobe the LH door jamb switch connector cavity to B+. Does the test lamp light? | -- | Go to Step 9 | Go to Step 10
5 |

1. Leave the J 35616-200 connected.
2. Disconnect the junction block connector C4.

Does the test lamp light?

--

Go to Step 7

Go to Step 8

6 | Replace the audio alarm module. Is the repair complete? | -- | Go to Audible Warnings System Check | --
7 | Test for a short to B+ using a J 39200 in the BLK/WHT wire between the junction block connector C4 cavity 3, the instrument panel cluster assembly connector C3 cavity 11and audio alarm module connector cavity 5. Is there a short to B+ in the BLK/WHT wire? | -- | Go to Step 11 | Go to Step 12
8 | Replace the junction block. Is the repair complete? | -- | Go to Audible Warnings System Check | --
9 | Repair the open in the BLK/BLU wire between the audio alarm module and the LH door jamb switch. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
10 |

1. Inspect for a poor ground connection at the LH door jamb switch.
2. If the connection is OK, replace the LH door jamb switch.

Is the repair complete?

--

Go to Audible Warnings System Check

--

11 | Repair the short to B+ in the BLK/WHT wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
12 | Replace the Instrument cluster printed circuit. Refer to Printed Instrument Cluster Circuit Replacement . Is the repair complete? | -- | Go to Audible Warnings System Check | --