For 1990-2009 cars

### Removal Procedure

1. Remove the fuel tank from the vehicle. Refer to Fuel Tank Replacement .
2. Disconnect the 2 vapor hoses (2) from the fill limiter vent valve (1).
3. Remove the 4 screws and the fill limiter vent valve from the fuel tank.

### Installation Procedures

1. Install the fill limiter vent valve to the fuel tank.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

2. Secure the fill limiter vent valve to the fuel tank with the 4 screws.

Tighten
Tighten the screws to 1.6 N·m (14 lb in).

3. Connect the 2 vapor hoses (2) to the fill limiter vent valve (1).