For 1990-2009 cars

## Rear Seat Back Cushion Cover and Pad Replacement Bench

### Removal Procedure

1. Remove the rear seat back. Refer to Rear Seat Back Replacement .
2. Remove the 2 plastic retaining clips from the lower outboard corners of the rear seat back.
3. Remove the 2 lock knobs (2) from the seat back (1).
4. Gently open the plastic seal (2) at the bottom of the seat back.
5. Roll the following components off of the seat back:

• | The rear seat back cover (3)

• | The carpet (1)

### Installation Procedure

1. Roll the following components onto the seat back:

• | The rear seat back cover (3)

• | The carpet (1)

2. Press the plastic seal (2) together along the bottom of the seat back.
3. Install 2 lock knobs (2) to the seat back (1). Secure the lock knobs by screwing in a clockwise direction.
4. Install 2 plastic retaining clips to the lower outboard corners of the rear seat back (1).
5. Install the rear seat back. Refer to Rear Seat Back Replacement .

## Rear Seat Back Cushion Cover and Pad Replacement Split

### Removal Procedure

1. Remove the rear seat back. Refer to Rear Seat Back Replacement .
2. Remove 2 plastic retaining clips from the lower outboard corners of the rear seat back.
3. Remove the lock knob (3) from the seat back (2 or 7).
4. Gently open the plastic seal (2) at the bottom of the seat back.
5. Roll the following components off of the seat back:

• | The rear seat back cover (3)

• | The carpet (1)

### Installation Procedure

1. Roll the following components onto the seat back:

• | The rear seat back cover (3)

• | The carpet (1)

2. Press the plastic seal (2) together along the bottom of the seat back.
3. Install the lock knob (3) to the seat back (2 or 7). Secure the knob by screwing in a clockwise direction.
4. Install the 2 plastic retaining clips to the lower outboard corners of the rear seat back (2 or 7).
5. Install the rear seat back. Refer to Rear Seat Back Replacement .