For 1990-2009 cars

# 1987 LABOR TIME GUIDE REVISIONS

Note the following additions and deletions to the 1987 Labor Time Guide:

#### LABOR OPERATION Z7000 (New Vehicle Inspection) :

SERIES VEHICLE LINE LABOR HOURS ------ ------------ ----------- A 6000 2.1

B Parisienne 2.3

F Firebird 2.3

G Grand Prix 2.3

H Bonneville 2.4

J Sunbird 2.0

N Grand Am 2.2

P Fiero 1.8

T T1000 1.9

In addition to the base time the following options requiring dealership installation will be covered by the additional allowances noted.

SERIES OPTION LABOR HOURS ------ ------ ----------- A Luggage Rack, Roof 0.5 B Luggage Rack, Roof 0.7 F (Trans Am Lower Frt. End Panel 0.7 Only) J Luggage Rack, Roof 0.2 A,B,G,H Locking Wire Wheel Covers 0.3

The labor operations listed below should be deleted from the 1987 microfiche as they are not applicable to the 1987 Bonneville.

LABOR OPERATION DESCRIPTION --------- ----------- D0500 Hose Aspirator - R & R or Replace D0520 Aspirator, Air Conditioning - Replace D0540 Sensor, In Car - Replace D0770 Programmer, Air Conditioning - R & R D0780 Programmer, Air Conditioning - Replace D1200 Sensor, Ambient - Replace D1210 Sensor, Outside Temperature - Replace

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.