For 1990-2009 cars

### Removal Procedure

1. Remove the front side door trim. Refer to Front Side Door Trim Panel Replacement in Doors.
2. Disconnect the front speaker electrical connector (3).
3. Remove the following components from the vehicle:

3.1. | 4 screws

3.2. | The speaker (2) and the housing (1) assembly

4. Remove the following components from the housing (2), if required:

4.1. | 4 screws

4.2. | The speaker (1)

### Installation Procedure

1. Install the speaker (1) to the housing (2), if removed. Secure the speaker with the 4 screws.
2. Install the speaker-housing assembly (1,2) to the door. Secure the assembly with the 4 screws.
3. Connect the front speaker electrical connector (3).
4. Install the front side door trim. Refer to Front Side Door Trim Panel Replacement in Doors.