For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Wiper/Washer Rear System Check
2 |

1. Turn the ignition switch to the ON position.
2. Backprobe the rear washer pump connector with a test lamp from cavity 1 to ground.
3. Press and hold the rear washer switch.

Does the test lamp light?

--

Go to Step 4

Go to Step 3

3 | Test for an open in the BLK/GRN wire between the rear wiper/washer switch and the rear washer pump. Was an open found? | -- | Go to Step 5 | Go to Step 6
4 | Test for an open in the BLK ground wire between the rear washer pump and G102. Was an open found? | -- | Go to Step 5 | Go to Step 7
5 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
6 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --
7 | Replace the rear washer pump. Refer to Rear Window Washer Pump Replacement . Is the repair complete? | -- | Go to Wiper/Washer Rear System Check | --