For 1990-2009 cars

### Removal Procedure

Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

1. Disconnect the negative battery cable.
2. Remove the 2 screws (1,7) which secure the composite headlamp/turn signal/parking lamp housing assembly (6).
3. Turn the parking/turn signal bulb (8) socket counterclockwise in order to remove the socket from the composite headlamp housing (6).
4. Remove the bulb (8) from the socket, if necessary.

### Installation Procedure

1. Install the bulb (8) to the socket, if removed.
2. Rotate the parking/turn signal bulb (8) socket clockwise in order to secure the socket to the headlamp housing (6).
3. Install the composite headlamp/turn signal/parking lamp housing assembly (6) to the vehicle. Secure the assembly with the 2 screws (1,7).
4. Connect the negative battery cable.
5. Adjust the composite headlamp aim. Refer to Headlamp Aiming .