For 1990-2009 cars

### Removal Procedure

Caution: This vehicle is equipped with a Supplemental Inflatable Restraint (SIR) System. Failure to follow the correct procedure could cause the following conditions:

• | Air bag deployment

• | Personal injury

• | Unnecessary SIR system repairs

In order to avoid the above conditions, observe the following guidelines:

• | Refer to SIR Component Views in order to determine if you are performing service on or near the SIR components or the SIR wiring.

• | If you are performing service on or near the SIR components or the SIR wiring, disable the SIR system. Refer to Disabling the SIR System.

1. Disable the SIR System. Refer to Disabling the SIR System in SIR.
2. Remove the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.
3. Disconnect the rear wiper/washer electrical connector.
4. Use a pick in order to push up on the clip on the bottom of the rear wiper/washer switch (9).
5. Remove the rear wiper/washer switch (9) from the left garnish trim panel (10).

### Installation Procedure

1. Connect the rear wiper/washer electrical connector.
2. Install the rear wiper/washer switch (9) to the left garnish trim panel (10). Push in the switch until the clip engages fully.
3. Install the knee bolster. Refer to Knee Bolster Replacement in Instrument Panel, Gauges and Console.
4. Enable the SIR System. Refer to Enabling the SIR System in SIR.