For 1990-2009 cars

The services shown in this schedule up to 166,000 km (100 000 miles) should be performed after 166 000 km (100,000 miles) at the same intervals.

### Footnotes

[Dagger] The U.S. Environmental Protection Agency or the California Air Resources Board has determined that the failure to perform this maintenance item will not nullify the emission warranty or limit recall liability prior to the completion of the vehicle's useful life. We, however, urge that all recommended maintenance services be performed at the indicated intervals and the maintenance be recorded.

# Lubricate the parking brake cable guides, underbody contact points and linkage.

+ A good time to check brakes is during tire rotation. Inspect the complete system. Inspect brake lines and hoses for proper hook-up, binding, leaks, cracks, chafing, etc. Inspect disc brake pads for wear and rotors for surface condition. Also inspect drum brake linings for wear and cracks. Inspect other brake parts, including drums, wheel cylinders, calipers parking brake, etc. Check parking brake adjustment. You may need to have your brakes inspected more often if your driving habits or conditions result in frequent braking.

### 5 000 km (3,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 10 000 km (6,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

### 15 000 km (9,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 20 000 km (12,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Change manual transaxle fluid (or every 12 months, whichever occurs first).

### 25 000 km (15,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Inspect air cleaner filter if your are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

• | Inspect the valve lash and adjust if necessary (1.3L Code 2 engine only).

• | Inspect fuel tank, cap and lines and any hoses for damage (or every 15 months, whichever occurs first). See footnote [Dagger].

### 30 000 km (18,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

### 35 000 km (21,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 40 000 km (24,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Change manual transaxle fluid (or every 12 months, whichever occurs first).

### 45 000 km (27,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 50 000 km (30,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Inspect engine accessory drive belts (or every 24 months, whichever occurs first).

• | Drain, flush and refill cooling system (or every 30 months, whichever occurs first). See Explanation of Scheduled Services for what to use. Inspect hoses. Clean radiator, condenser, pressure cap and neck. Pressure test the cooling system and pressure cap. See footnote [Dagger].

• | Replace spark plugs.

• | Replace air cleaner filter.

• | Inspect valve lash and adjust if necessary (1.3L Code 2 engine only).

• | Inspect fuel tank, cap and lines and any hoses for damage, (or every 15 months, whichever occurs first). See footnote [Dagger]

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

### 55 000 km (33,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 60 000 km (36,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Change manual transaxle fluid (or every 12 months, whichever occurs first).

### 65 000 km (39,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 70 000 km (42,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

### 75 000 km (45,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Inspect air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

• | Inspect the valve lash and adjust if necessary (1.3L Code 2 engine only).

• | Inspect fuel tank, cap and lines and any hoses for damage, (or every 15 months, whichever occurs first). See footnote [Dagger].

### 80 000 km (48,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Change manual transaxle fluid (or every 12 months, whichever occurs first).

### 83 000 km (50,000 Miles)

Change automatic transaxle fluid and filter if the vehicle is mainly driven under one or more of these conditions:

• | In heavy city traffic where the outside temperature regularly reaches 90°F (32°C) or higher.

• | In hilly or mountainous terrain.

• | Uses such as found in taxi, police or delivery service.

• | If vehicle is not used under any of these conditions, the fluid and filter do not require changing.

### 85 000 km (51,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 90 000 km (54,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

### 95 000 km (57,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 100 000 km (60,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Inspect engine accessory drive belts (or every 24 months, whichever occurs first).

• | Inspect camshaft timing belt. See footnote [Dagger].

• | Drain, flush and refill cooling system (or every 30 months, whichever occurs first). See Explanation of Scheduled Services for what to use. Inspect hoses. Clean radiator, condenser, pressure cap and neck. pressure test the cooling system and pressure cap. See footnote [Dagger].

• | Replace spark plugs.

• | Replace spark plug wires (or every 60 months, whichever occurs first).

• | Inspect underhood wiring harness for loose connections, chafed wires and damage (or every 60 months, whichever occurs first). See footnote [Dagger].

• | Drain, refill and bleed the brake system.

• | Replace air cleaner filter.

• | Inspect the valve lash and adjust if necessary (1.3L Code 2 engine only

• | Inspect fuel tank, cap and lines and any hoses for damage (or every 15 months, whichever occurs first). See footnote [Dagger].

• | Change manual transaxle fluid (or every 12 months, whichever occurs first).

• | Rotate tires. See Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

### 105 000 km (63,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 110 000 km (66,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

### 115 000 km (69,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 120 000 km (72,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Change manual transaxle fluid (or every 12 months, whichever occurs first).

### 125 000 km (75,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Inspect air cleaner filter if you are driving in dusty conditions. Replace filter if necessary. See footnote [Dagger].

• | Inspect the valve lash and adjust if necessary (1.3L Code 2 engine only).

• | Inspect fuel tank, cap and lines and any hoses for damage (or every 15 months, whichever occurs first). See footnote [Dagger].

### 130 000 km (78,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

### 135 000 km (81,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 140 000 km (84,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Change manual transaxle fluid (or every 12 months, whichever occurs first).

### 145 000 km (87,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 150 000 km (90,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Inspect engine accessory drive belts (or every 24 months, whichever occurs first).

• | Drain, flush and refill cooling system (or every 30 months, whichever occurs first). See Explanation of Scheduled Services for what to use. Inspect hoses. Clean radiator, condenser, pressure cap and neck. Pressure test the cooling system and pressure cap. See footnote [Dagger].

• | Replace spark plugs.

• | Replace air cleaner filter.

• | Inspect the valve lash and adjust if necessary (1.3L Code 2 engine only).

• | Inspect fuel tank, cap, cap gasket and lines for damage (or every 15 months, whichever occurs first). See footnote [Dagger].

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

### 155 000 km (93,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 160 000 km (96,000 Miles)

• | Change engine oil and filter (or every 3 months, whichever occurs first).

• | Lubricate chassis components (or every 6 months, whichever occurs first). See footnote #.

• | Rotate tires. Refer to Explanation of Scheduled Services for proper rotation pattern and additional information. See footnote +.

• | Change manual transaxle fluid (or every 12 months, whichever occurs first).

### 165 000 km (99,000 Miles)

Change engine oil and filter (or every 3 months, whichever occurs first).

### 166 000 km (100,000 Miles)

• | Change automatic transaxle fluid and filter if the vehicle is mainly driven under one or more of these conditions:

- | In heavy city traffic where the outside temperature regularly reaches 90°F (32°C) or higher.

- | In hilly or mountainous terrain.

- | Uses such as found in taxi, police or delivery service.

- | If vehicle is not used under any of these conditions, the fluid and filter do not require changing.

• | Replace fuel filter.

• | Replace camshaft timing belt.

### 200 000 km (120,00 Miles)

Replace evaporative emission canister air suction filter (1.3L Code 2 engine only).