For 1990-2009 cars

### Removal Procedure

1. Remove the rear door window. Refer to Rear Side Door Window Replacement .
2. Remove the rear door outer garnish (1) from the rear door by removing the 3 screws.
3. Remove the 1 screw that secures the outer sealing strip (7) to the rear door.
4. Unclip the 4 clips and remove the outer sealing strip (7) from the door.

### Installation Procedure

1. Clip the outer sealing strip (7) into place.
2. Secure the outer sealing strip (7) to the door with the 1 screw.
3. Install the rear door outer garnish (1) to the rear door. Secure the garnish with the 3 screws.
4. Install the rear door window. Refer to Rear Side Door Window Replacement .