For 1990-2009 cars

## Front Side Door Window Front Channel and Rear Channel Replacement Front

### Removal Procedure

1. Remove the front door window. Refer to Front Side Door Window Replacement .
2. Remove the front radio speaker and the bracket. Refer to Radio Front Speaker Replacement in Entertainment.
3. Position the front door water deflector aside in order to gain access to the screws (2) and to the front window channel (3).
4. Remove the door window weather strip (1) from the front window channel (3).
5. Remove the front window channel (3) from the front door by removing the 2 screws (2).

### Installation Procedure

1. Install the front window channel (3) to the front door. Secure the channel with the 2 screws (2).
2. Install the door window weather strip (1) to the front window channel (3).
3. Install the front radio speaker and the bracket. Refer to Radio Front Speaker Replacement in Entertainment.
4. Install the front door window. Refer to Front Side Door Window Replacement .

## Front Side Door Window Front Channel and Rear Channel Replacement Rear

### Removal Procedure

1. Remove the front door window. Refer to Front Side Door Window Replacement .
2. Position the front door water deflector aside in order to gain access to the screws and the rear window channel (2).
3. Remove the door window weather strip from the rear window channel (2).
4. Remove the rear window channel (2) from the front door by removing the 2 screws.

### Installation Procedure

1. Install the rear window channel (2) to the front door. Secure the channel with the 2 screws.
2. Install the door window weather strip to the rear window channel (2).
3. Install the front door window. Refer to Front Side Door Window Replacement .