For 1990-2009 cars

### Removal Procedure

1. Discharge and recover the refrigerant. Refer to Refrigerant Recovery and Recharging .
2. Remove the bolt and the inlet tube from the top of the receiver-dryer (5).
3. Disconnect the receiver-dryer inlet from the condenser outlet pipe fitting (6).

### Installation Procedure

1. Coat new O-rings with mineral base 525 viscosity refrigerant oil.
2. Install the O-rings to the receiver-dryer inlet tube.
3. Install the inlet tube to the top of the receiver-dryer (5). Secure inlet tube with the bolt.
4. Connect the receiver-dryer inlet to the condenser outlet pipe fitting (6).
5. Evacuate and recharge the air conditioning (A/C) system. Refer to Refrigerant Recovery and Recharging .
6. Operate the A/C system, and test the system for refrigerant leaks. Refer to Leak Testing .