For 1990-2009 cars

### Removal Procedure

1. Gently pry off the inner mirror garnish (8).
2. Remove the following components from the door by removing the following items:

2.1. | Three screws

2.2. | The mirror assembly (7)

2.3. | The mirror gasket

3. Remove the outer mirror bezel from the door.

### Installation Procedure

1. Install the gasket to the mirror (7).
2. Install the mirror assembly (7) to the door. Secure the mirror with the 3 screws.
3. Snap the inner mirror garnish (8) into place on the door.