For 1990-2009 cars

Causes | Correction
--- | ---
Incorrect front wheel alignment | Set the front end alignment to specification.
Contaminated brake linings | Replace the brake linings.
Incorrect tire pressure | Set the tire pressure to specification.
Loose front suspension parts | Locate and tighten, repair or replace the loose front suspension components.
Contaminated or improper brake fluid | Flush the brake system and repair the affected brake components.
Worn out brake linings | Replace the brake linings.
Uneven brake lining material | Replace the brake linings.
Glazed brake linings | Replace the brake linings.
Incorrect lining material | Replace the brake linings.
Lining damaged by abusive use | Replace the brake linings.
Scored rotor | Refinish the rotor surface or replace the rotor.
Loose front or rear brake assembly attachment | Locate and tighten the loose brake components.
Restricted brake fluid passage | Locate and repair the source of the brake fluid restriction.
Leaking brake pipe or connection | Locate and repair the brake pipe or the connection.
Leaking piston seal | Replace the caliper piston seal
Sticky caliper or caliper pistons | Repair or replace the caliper.
Parking brake not releasing | Repair the malfunctioning park brake lever or frozen parking brake cables.
Improper caliper to knuckle clearance | Repair as necessary.
Improper rotor surface finish | Refinsh the rotor surface or replace the rotor.