For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the underhood Electrical Center cover.
3. Remove the Electronic Brake Control Relay (2) from the underhood electrical center (1).

### Installation Procedure

1. Install the Electronic Brake Control Relay (2) into the underhood electrical center (1).
2. Install the underhood Electrical Center cover.
3. Close the hood.
4. Perform the A Diagnostic System Check - ABS .