For 1990-2009 cars

The condition of an automatic transaxle not operating properly may be influenced by one or a combination of the following items:

• | The fluid level may be too high or too low. Refer to Fluid Leak Diagnosis and Repair .

• | The engine may be performing poorly. Refer to Engine Controls.

• | The throttle valve (TV) cable may be out of adjustment. Refer to Automatic Transmission Throttle Valve Cable Adjustment .

• | The shift select cable may be out of adjustment. Refer to Range Selector Lever Cable Replacement .

• | The transaxle may have internal fluid leaks. Refer to the Transmission Unit Repair Manual.

• | There may be a problem with the electrical system. Refer to Engine Electrical.

• | The vehicle may have a problem in the transaxle or in the other mechanical components.