For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Radio/Audio System Check
2 | Inspect the tape player door for an obstruction. Is an obstruction present? | -- | Go to Step 3 | Go to Step 4
3 | Remove the obstruction. Is the repair complete? | -- | Go to Step 5 | --
4 | Remove the radio for repair. Refer to Radio Replacement . Is the repair complete? | -- | Go to Radio/Audio System Check | --
5 |

1. Inspect and clean the tape head
2. Insert the diagnostic test tape.

Does the tape player operate properly?

--

Go to Radio/Audio System Check

Go to Step 6

6 | Remove the radio for repair. Refer to Radio Replacement . Is the repair complete? | -- | Go to Radio/Audio System Check | --