For 1990-2009 cars

# Warranty Admin. - September, 2000 Labor Time Guide Updates

Subject: | September, 2000 Labor Time Guide Updates

Models: | 1996-2001 Passenger Cars and Trucks

This bulletin addresses changes to the published General Motors Labor Time Guides. These changes (new or revised) are the result of new time studies and/or dealer "Requests For Review" being handled by the GM Service Operations Group. They are effective upon receipt. All changes will appear in the next printing of the Labor Time Guide.

#### LTG Update - C/K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
ROTOR ASSEMBLY - R&R OR REPLACE

- NOTE: No Change to "PART GP", "INC" or Labor Operations H0120, H0121, H0130, H0131, or H0137.

FRONT |  |  |  |  |  |  |  |
BOTH |  | H0127 |  |  |  |  |  |
C TRUCK EXCEPT 3500 HD |  |  | 1.2 | 1.2 | 1.2 | 1.2 | 1.2 |
C TRUCK 3500 HD | R |  | 1.4 | 1.4 | 1.4 | 1.4 | 1.4 | 1.4
K TRUCK (UNDER 8600 GVW) |  |  | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 |
K TRUCK (OVER 8600 GVW) |  |  | 2.2 | 2.2 | 2.2 | 2.2 | 2.2 |

- No Change to "ADD" Conditions

PLUG, TRANSFER CASE DRAIN - REPLACE

- INC: Adjust fluid level as necessary

R

K4290

0.3

0.3

0.3

0.3

0.3

0.3

PLUG, TRANSFER CASE FILL - REPLACE | R | K4291 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
*IND: N - New/R - Revised

#### LTG Update - C/K - New Body Style - Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
REGULATOR, REAR DOOR WINDOW - R&R OR REPLACE

- NOTE: No Change to "PART GP", "INCs" or Labor Operations C0380 and C0381.

- NOTE: Regulator includes motor

R

RIGHT POWER |  | C0382 | -- | -- | -- | 0.5 | 0.5 | 0.5
LEFT POWER |  | C0383 | -- | -- | -- | 0.5 | 0.5 | 0.5
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

N

--

--

--

0-0.3

0-0.3

0-0.3

CASE, IGNITION LOCK CYLINDER (PASSLOCK SENSOR) - REPLACE

- INC: Passlock relearn.

- NOTE: Includes disable SIR System

R

E7202

--

--

--

1.3

1.3

1.3

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

N

--

--

--

0-0.3

0-0.3

0-0.3

SENSOR ASSEMBLY, IGNITION LOCK (PASSLOCK) - REPLACE |  | E7450 | THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS
SHOE, REAR DISC PARKING BRAKE - REPLACE |  |  |  |  |  |  |  |
RIGHT | R | H3050 |  |  |  |  |  |
1500 SERIES |  |  | -- | -- | -- | 1.0 | 1.0 | 1.0
2500 SERIES |  |  | -- | -- | -- | 0.6 | 0.6 | 0.6
LEFT | R | H3051 |  |  |  |  |  |
1500 SERIES |  |  | -- | -- | -- | 1.0 | 1.0 | 1.0
2500 SERIES |  |  | -- | -- | -- | 0.6 | 0.6 | 0.6
BOTH | R | H3052 |  |  |  |  |  |
1500 SERIES |  |  | -- | -- | -- | 1.3 | 1.3 | 1.3
2500 SERIES |  |  | -- | -- | -- | 0.9 | 0.9 | 0.9
LIFTER, VALVE - REPLACE

- PART GP: 0.459

- NOTE: Applies to V8 Engine, Codes V, T, U

ONE CYL |  |  |  |  |  |  |  |
RIGHT BANK |  | J0620 | -- | -- | -- | 3.7 | 3.7 | 3.7
LEFT BANK |  | J0621 | -- | -- | -- | 4.4 | 4.4 | 4.4
BOTH BANKS |  | J0627 | -- | -- | -- | 5.7 | 5.7 | 5.7
ADD: |  |  |  |  |  |  |  |

- A- Replace All Lifters

- Right or Left

--

--

--

0.2

0.2

0.2

- Both

--

--

--

0.4

0.4

0.4

- B- To Clean Parts On Vehicles Over 30,000 Miles/48,000 Kilometers If Nec

- Right or Left

--

--

--

0.3

0.3

0.3

- Both

--

--

--

0.4

0.4

0.4

- C- With Hydraulic Brake Booster

N

--

--

--

0.1

0.1

0.1

PLUG TRANSFER CASE DRAIN - REPLACE

- INC: Adjust fluid level as necessary

R

K4290

--

--

--

0.3

0.3

0.3

FILTER, AUXILLARY TRANSMISSION OIL - SPIN-ON - REPLACE

- NOTE: Applies to Allison Automatic Transmission

N

K5281

--

--

--

--

--

0.3

MODULATOR AND/OR SEAL - REPLACE

- NOTE: Applies to Allison Automatic Transmission

K6180

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

SENSOR, VEHICLE SPEED - REPLACE

- NOTE: Applies to Allison Automatic Transmission

K6310

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

SENSOR ASSEMBLY, SPEED INPUT - REPLACE

- NOTE: Applies to Allison Automatic Transmission

N

K6311

--

--

--

--

--

0.3

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

--

--

0-0.3

SENSOR ASSEMBLY, SPEED OUTPUT - REPLACE

- NOTE: Applies to Allison Automatic Transmission

N

K6312

--

--

--

--

--

0.3

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

--

--

0-0.3

SENSOR ASSEMBLY, TURBINE SPEED - REPLACE

- NOTE: Applies to Allison Automatic Transmission

N

K6315

--

--

--

--

--

0.3

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

--

--

0-0.3

PAN AND/OR GASKET, TRANSMISSION OIL - REPLACE

- INC: Filter or strainer

- NOTE: Applies to Allison Automatic Transmission

N

K6500

--

--

--

--

--

0.8

SOLENOIDS, A/B SHIFT - REPLACE

- NOTE: A/B trim solenoid.

- NOTE: Applies to Allison Automatic Transmission

N

K6523

--

--

--

--

--

1.1

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

N

--

--

--

--

--

0-0.3

SOLENOID, ON/OFF - REPLACE

- NOTE: Applies to Allison Automatic Transmission

- NOTE: Solenoids C, D, E

N

K6558

--

--

--

--

--

1.0

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

--

--

0-0.3

SOLENOID, TORQUE CONVERTER CLUTCH - REPLACE

- NOTE: Applies to Allison Automatic Transmission

- NOTE: Solenoid F

N

K6567

--

--

--

--

--

1.0

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

--

--

0-0.3

PUMP AND/OR GASKET, TRANSMISSION OIL - REPLACE

- NOTE: Applies to Allison Automatic Transmission

K7120

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

FRONT CLUTCH, REAR CLUTCH, BRAKE BAND - REPLACE

- NOTE: Applies to Allison Automatic Transmission

K7210

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

INTERNAL GEAR, FRONT CARRIER, SUN GEAR, CONNECTING SHELL - REPLACE

- NOTE: Applies to Allison Automatic Transmission

K7545

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

DRIVE HUB, INTERNAL GEAR, PARKING GEAR - REPLACE

- NOTE: Applies to Allison Automatic Transmission

K7570

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

ONE WAY CLUTCH, REAR CARRIER - REPLACE

- NOTE: Applies to Allison Automatic Transmission

K7575

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

CLUTCH LOW AND REVERSE - REPLACE

- NOTE: Applies to Allison Automatic Transmission

K7580

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

CASE, TRANSMISSION - REPLACE

- NOTE: Applies to Allison Automatic Transmission

K7800

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

TRANSMISSION ASSEMBLY - RECONDITION

- NOTE: Applies to Allison Automatic Transmission

K7900

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

*IND: N - New/R - Revised

#### LTG Update - F Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
AIR CONDITIONING MODULE COMPONENTS - R&R OR REPLACE

- NOTE: No Change to "PART GP" or "POLICY"

SEAL, HVAC MODULE TO BODY | N | D2118 | -- | -- | -- | -- | 0.6 | 0.6
ADD: |  |  |  |  |  |  |  |

- A- To Recover/Recharge A/C System

0.5

0.5

0.5

0.5

0.5

0.5

- B- Remove T-Tops

--

--

--

--

0.1

0.1

*IND: N - New/R - Revised

#### LTG Update - G Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PUMP, SECONDARY AIR INJECTION - REPLACE | N | J6050 | -- | -- | -- | -- | -- | 0.5
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

--

--

0-0.3

SOLENOID, SAI VACUUM CONTROL - REPLACE | N | J6096 | -- | -- | -- | -- | -- | 0.2
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

--

--

0-0.3

*IND: N - New/R - Revised

#### LTG Update - H Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
ADJUSTER ASSEMBLY, FRONT SEAT MANUAL - R&R OR REPLACE

- NOTE: No Change to "PART GP" or Labor Operation C6021

SPLIT/DIVIDED SEAT PASSENGER |  | C6020 |  |  |  |  |  |

- ONE SIDE

R

0.4

0.4

0.4

0.4

1.2

1.2

- No Change to "ADD" Condition.

*IND: N - New/R - Revised

#### LTG Update - J Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
NOTE:

- The labor times published in the August LTG Update Bulletin #00-00-89-017 under the 4T40-E Automatic Transaxle pertaining to Engine Code 4 apply to model years 1996 through 2001.

N

CLUTCH & CONTROLS

- The following "NOTE" has been deleted and no longer applies to any applicable labor operation within the Clutch & Controls section of the current labor time guide.

- NOTE: For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

TRANSMISSION 5-SPEED

- The following "NOTE" has been deleted and no longer applies to any applicable labor operation within the Transmission 5-Speed section of the current labor time guide.

- NOTE: For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

AUTOMATIC TRANSAXLE HYDRA-MATIC 3T40

- The following "NOTE" has been deleted and no longer applies to any applicable labor operation within the Automatic Transaxle Hydra-matic 3T40 section of the current labor time guide.

- NOTE: For check & adjust toe-in, refer to operation E2000 and add the applicable times to the regular hours column.

R

*IND: N - New/R - Revised

#### LTG Update - K Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CARRIER AND DIFFERENTIAL FINAL DRIVE ASSEMBLY, FINAL DRIVE SUN GEAR, PARKING GEAR AND FINAL DRIVE INTERNAL GEAR - R&R OR REPLACE

- NOTE: Applies to Auto Trans 4T80E

- NOTE: No Change to Labor Operations K6395, K6396 or K6397

FINAL DRIVE INTERNAL GEAR | R | K6399 | -- | -- | 3.6 | 3.6 | 3.6 | 3.6
MODULE - REPLACE

- NOTE: No Change to Labor Operations N4823, N4833, N4851, N4852, N4853, N4855, N4857, N4858 or N4859

DASH INTEGRATION | R | N4862 | -- | -- | 0.5 | 0.5 | 0.5 | 0.5

- No Change to "ADD" Condition

PRE-DELIVERY INSPECTION - BASE TIME |  | Z7000 | -- | -- | 1.6 | 1.6 | 1.6 | 1.6
ADD: |  |  |  |  |  |  |  |

- A- To Install Cellular Phone (RPO UV8) INC: Additional time for steering wheel controls.

R

--

--

--

--

2.5

2.5

*IND: N - New/R - Revised

#### LTG Update - Ksp Platform

OPERATION DESCRIPTION -- | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PLATE, INSTRUMENT PANEL TRIM - R&R OR REPLACE

- PART GP: 10.252

RIGHT | R | C2320 | 1.1 | 1.1 | 1.1 | 1.1 | 1.1 | 1.1
LEFT |  | C2321 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6 | 0.6
PRE-DELIVERY INSPECTION - BASE TIME |  | Z7000 | -- | -- | 1.6 | 1.6 | 1.6 | 1.6
ADD: |  |  |  |  |  |  |  |

- A- To Install Cellular Phone (RPO UV8) INC: Additional time for steering wheel controls.

R

- W/Full console

--

--

--

--

2.5

2.5

- W/Flex console

--

--

--

--

1.8

1.8

*IND: N - New/R - Revised

#### LTG Update - M/L Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PLUG, TRANSFER CASE DRAIN - REPLACE

- INC: Adjust fluid level as necessary

R

K4290

0.3

0.3

0.3

0.3

0.3

0.3

PLUG, TRANSFER CASE FILL - REPLACE | N | K4291 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
*IND: N - New/R - Revised

#### LTG Update - N Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MOLDING AND/OR OUTER STRIP, REAR DOOR WINDOW REVEAL - R&R OR REPLACE

- PART GP: 10.772

RIGHT |  |  |  |  |  |  |  |
GRAND AM & ALERO | R | B7920 | 0.2 | 0.2 | 0.2 | 0.2 | 0.6 | 0.6
LEFT |  |  |  |  |  |  |  |
GRAND AM & ALERO | R | B7921 | 0.2 | 0.2 | 0.2 | 0.2 | 0.6 | 0.6
SPEAKER, RADIO - REPLACE

- NOTE: No Change to "PART GP" or Labor Operations R0940, R0941, R0944, R0945 or R0948

REAR |  |  |  |  |  |  |  |
RIGHT |  | R0950 |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
ACHIEVA & SKYLARK |  |  | 0.8 | 0.8 | 0.8 |  |  |
GRAND AM & ALERO | R |  | 0.8 | 0.8 | 0.8 | 0.4 | 0.4 | 0.4
REAR |  |  |  |  |  |  |  |
LEFT |  | R0951 |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
ACHIEVA & SKYLARK |  |  | 0.8 | 0.8 | 0.8 |  |  |
GRAND AM & ALERO | R |  | 0.8 | 0.8 | 0.8 | 0.4 | 0.4 | 0.4
REAR |  |  |  |  |  |  |  |
BOTH |  | R0958 |  |  |  |  |  |
MALIBU & CUTLASS |  |  | -- | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
ACHIEVA & SKYLARK |  |  | 0.8 | 0.8 | 0.8 |  |  |
GRAND AM & ALERO | R |  | 0.8 | 0.8 | 0.8 | 0.5 | 0.5 | 0.5

- No Change to "ADD" Condition

*IND: N - New/R - Revised

#### LTG Update - S Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
PANEL, SUNROOF - ALIGN. | N | B2720 | -- | -- | 0.3 | 0.3 | 0.3 | 0.3
*IND: N - New/R - Revised

#### LTG Update - S/T Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CORE, HEATER - REPLACE

- NOTE: No Change to "PART GP", "INC", or Labor Operation D2820

A/C | R | D2822 |  |  |  |  |  |
LEFT HAND DRIVE |  |  |  |  |  |  |  |
UTILITY |  |  | 3.7 | 3.7 | 3.7 | 3.7 | 3.7 | 3.7
PICK-UP |  |  | 3.7 | 3.7 | 3.7 | 3.7 | 3.7 | 3.7
RIGHT HAND DRIVE |  |  | -- | -- | -- | 5.4 | 5.4 | 5.4

- No Change to "ADD" Condition

CASE, IGNITION LOCK CYLINDER (PASSLOCK SENSOR) - REPLACE

- INC: Passlock relearn

- NOTE: Includes disable SIR System

N

E7202

--

--

--

1.3

1.3

1.3

ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis.

--

--

--

0-0.3

0-0.3

0-0.3

SENSOR ASSEMBLY, IGNITION LOCK (PASSLOCK) - REPLACE

- INC: Disable and Enable SIR System

E7450

THIS LABOR OPERATION HAS BEEN DELETED FROM ALL APPLICABLE YEARS

PLUG, TRANSFER CASE DRAIN - REPLACE

- INC: Adjust fluid level as necessary

R

K4290

0.3

0.3

0.3

0.3

0.3

0.3

PLUG, TRANSFER CASE FILL - REPLACE | R | K4291 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2 | 0.2
LAMP ASSEMBLY - REPLACE

- NOTE: No Change to "INCs", or Labor Operations N4120, N1440, N1441, N1456, N1466, N1467, N1477, N1524, N1525, N1530, N1564, N1565, N1600 or N1610

PARK AND TURN SIGNAL |  |  |  |  |  |  |  |
RIGHT | R | N1520 | 1.2 | 1.2 | 0.3 | 0.3 | 0.3 | 0.3
LEFT |  | N1521 | 1.2 | 1.2 | 0.3 | 0.3 | 0.3 | 0.3
RECEIVER, RADIO

- NOTE: No Change to "PART GP", "NOTES" or Labor Operation R0760

REMOVE RADIO |  | R0762 |  |  |  |  |  |
LEFT HAND DRIVE | R |  | 1.0 | 1.0 | 0.3 | 0.3 | 0.3 | 0.3
RIGHT HAND DRIVE |  |  | -- | -- | -- | 0.6 | 0.6 | 0.6
REINSTALL RADIO |  | R0763 |  |  |  |  |  |
LEFT HAND DRIVE | R |  | 1.0 | 1.0 | 0.3 | 0.3 | 0.3 | 0.3
RIGHT HAND DRIVE |  |  | -- | -- | -- | 0.6 | 0.6 | 0.6

- No Change to "ADD" Conditions

*IND: N - New/R - Revised

#### LTG Update - U/X Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
MODULE, EXPRESS SUNROOF - REPLACE | N | N4833 | 1.4 | 1.4 |  |  |  |
ADD: |  |  |  |  |  |  |  |

- A- Diagnosis Time: You may claim 0.0 to 0.3 hours depending on actual time performing diagnosis

0-0.3

0-0.3

*IND: N - New/R - Revised

#### LTG Update - W Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
CORE, EVAPORATOR - REPLACE

- PART GP: 9.210

D3320

CHEVROLET |  |  |  |  |  |  |  |
LUMINA |  |  | 2.1 | 2.1 | 2.1 | 2.1 | 2.1 | 2.1
MONTE CARLO |  |  | 2.1 | 2.1 | 2.1 | 2.1 | 6.0 | 6.0
IMPALA |  |  | -- | -- | -- | -- | 6.0 | 6.0
PONTIAC/BUICK | R |  | 4.0 | 6.0 | 6.0 | 6.0 | 6.0 | 6.0
OLDSMOBILE |  |  | 2.1 | 2.1 | 5.8 | 5.8 | 5.8 | 5.8
ENGINE CODE X |  |  | 4.2 | 4.2 |  |  |  |
ADD: |  |  |  |  |  |  |  |

- A- Recover/Recharge A/C System

0.5

0.5

0.5

0.5

0.5

0.5

- B- To R&R Center Console

R

0.4

0.2

0.2

0.2

0.2

0.2

TANK, FUEL - REPLACE

- NOTE: No change to "PART GP" or "POLICY"

L1260

CHEVROLET LUMINA | R |  | 1.5 | 1.5 | 1.5 | 1.5 | 1.5 | 1.5
CHEVROLET IMPALA & MONTE CARLO | R |  | 1.5 | 1.5 | 1.5 | 1.5 | 1.9 | 1.9
PONTIAC | R |  | 1.5 | 1.8 | 1.8 | 1.8 | 1.8 | 1.9
OLDSMOBILE | R |  | 1.5 | 1.5 | 1.8 | 1.8 | 1.8 | 1.9
BUICK | R |  | 1.5 | 1.8 | 1.8 | 1.8 | 1.9 | 1.9
*IND: N - New/R - Revised

#### LTG Update - Y Platform

OPERATION DESCRIPTION | IND* | OP NUM | MODEL YEAR
--- | --- | --- | ---
96 | 97 | 98 | 99 | 00 | 01
YEAR VIN CODE
T | V | W | X | Y | 1
VALVE, SAI CHECK - REPLACE

- PART GP: 3.670

- POLICY: E

- NOTE: Applies to V8 Engine, Codes G, P and 5

ONE |  | J6086 | 0.3 |  |  |  |  |
RIGHT | R | J6090 | -- | 1.7 | 1.7 | 1.7 | 1.7 | 1.7
LEFT |  | J6091 | -- | 0.3 | 0.3 | 0.3 | 0.3 | 0.3
ADD: |  |  |  |  |  |  |  |

- No Change to "ADD" Condition

*IND: N - New/R - Revised