For 1990-2009 cars

# SPARK PLUG GAPS AND USAGE NOT ON EMISSION LABEL

1985 AND 1986 ENIGNES USED ON ALL PONTIAC CARLINES

"Please discard previous bulletin 86-6(Gasoline)-10A and replace with 86-6(Gasoline)-10B due to text revision."

Emission labels used on 1985-1986 Pontiac Carlines no longer inclUde spark Plug gap information. Following is a list of correct spark plug gaps for all 1985-1986 engines: (For spark plug gap information in model years 1981 through 1984, see bulletin 85-6-11.)

ENGINE 1985 1986 ------ ---- ---- VIN DISPL. PLUG GAP PLUG GAP --- ----- ---- --- ---- --- C 1.6L R42CTS .035 R42CTS .035 O 1.8L R44XLS .035 R44XLS .035 J 1.8L R42CXLS .035 R42CXLS .035 P 2.0L R42CTS .035 R42CTS .035 2 2.5L R43TSX .060 R43CTS6 .060 R 2.5L R43TSX .060 R43CTS6 .060 U 2.5L R43TSX .060 R43CTS6 .060 X 2.8L R43CTS .045 R43CTS .045 W 2.8L R42CTS .045 R42CTS .045 S 2.8L R42CTS .045 R42CTS .045 9 2.8L R42CTS .045 R42CTS .045 L 3.0L R44LTS .040 R44LTS .045 A 3.8L R45TSX .060 R45TSX .060 Z 4.3L R43CTS .035 R43CTS .035 H 5.0L R45TS .045 R43TS .035 G 5.0L R44TS .045 R43CTS .035 F 5.0L R43CTS .045 R43CTS .035 Y 5.0L --- ---- FR3LS6 .060

General Motors bulletins are intended for use by professional technicians, not a "do-it-yourselfer". They are written to inform those technicians of conditions that may occur on some vehicles, or to provide information that could assist in the proper service of a vehicle. Properly trained technicians have the equipment, tools, safety instructions and know-how to do a job properly and safely. If a condition is described, do not assume that the bulletin applies to your vehicle, or that your vehicle will have that condition. See a General Motors dealer servicing your brand of General Motors vehicle for information on whether your vehicle may benefit from the information.