For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the water deflector (1) from the door.

### Installation Procedure

1. Apply adhesive to the back of the water deflector (1).
2. Install the water deflector (1) to the door.
3. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .