For 1990-2009 cars

Step | Action | Normal Result(s) | Abnormal Result(s)*
--- | --- | --- | ---
1 |

1. Turn the ignition switch to the ON position.
2. Press and hold the rear wiper/washer switch.

1. The rear washer pump operates.
2. The rear wiper operates.

• | Rear Wiper Inoperative

• | Rear Washer Inoperative

• | Wipers On Mode Inoperative - Rear

2 | Release the rear washer switch. | The following components stop in the PARK position:

• | The washer pump

• | The rear wiper

• | Rear Wiper Always On

• | Rear Wiper Blade Does Not Park

3 | Press the rear wiper switch to the ON position. | The rear wiper operates. | Rear Wiper Inoperative
4 | Press the rear wiper switch to the OFF position. | The rear wiper completes the cycle and returns to the PARK position. |

• | Rear Wiper Always On

• | Rear Wiper Blade Does Not Park

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.