For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Air Cleaner-to-Cylinder Head Bolt | 10 N·m | 89 lb in
A/C Compressor Drive Belt Tensioner | 45 N·m | 33 lb ft
Battery Cable Nut | 15 N·m | 11 lb ft
Connecting Rod Bearing Cap Nuts | 35 N·m | 26 lb ft
Camshaft Housing Bolts | 11 N·m | 97 lb in
Camshaft Timing Gear Bolt | 60 N·m | 44 lb ft
Coolant Pump Pulley Bolts | 24 N·m | 18 lb ft
Crankshaft Pulley Bolts | 16 N·m | 12 lb ft
Crankshaft Timing Gear Bolt | 130 N·m | 96 lb ft
Cylinder Head-to-Engine Block Bolts | 73 N·m | 54 lb ft
Valve Rocker Arm Cover Nuts | 5 N·m | 44 lb in
Engine Oil Drain Plug | 35 N·m | 26 lb ft
Engine Oil Pan Bolts and Nuts | 11 N·m | 97 lb in
Exhaust Manifold Bolts and Nuts | 23 N·m | 17 lb ft
Exhaust Manifold Stiffener Bracket Bolts | 50 N·m | 37 lb ft
Exhaust Manifold-to-Front Pipe/Three Way Catalytic Converter (TWC) Assembly Bolts | 45 N·m | 33 lb ft
Flywheel Retaining Bolts | 75 N·m | 55 lb ft
Generator Mounting Bolts and Nuts | 23 N·m | 17 lb ft
Guide Tube Bolt | 11 N·m | 97 lb in
Heat Shield Bolts | 15 N·m | 11 lb ft
Heated Oxygen Sensor | 40-50 N·m | 29-36 lb ft
Intake Manifold Mounting Bolts | 23 N·m | 17 lb ft
Lower Generator Cover Bolts | 5.5 N·m | 49 lb in
Main Bearing Bolts | 54 N·m | 40 lb ft
Oil Pressure Switch | 14 N·m | 10 lb ft
Oil Pump Mounting Bolts | 11 N·m | 97 lb in
Oil Pump Strainer Bolt | 11 N·m | 97 lb in
Oil Pump Strainer Bracket Bolt | 11 N·m | 97 lb in
Rear Engine Mount Through Bolt and Nut | 55 N·m | 41 lb ft
Rear Engine Mount-to-Bulkhead Bolts | 55 N·m | 41 lb ft
Rear Main Seal Housing Bolts | 12 N·m | 106 lb in
Resonator/Muffler/Tail Pipe Assembly-to-Front Pipe/Three Way Catalytic Convert (TWC) Assembly Nuts | 40 N·m | 29 lb ft
Timing Belt Cover Nut and Bolts | 11 N·m | 97 lb in
Timing Belt Tensioner Bolt | 27 N·m | 20 lb ft
Timing Belt Tensioner Stud | 11 N·m | 97 lb in
Torque Rod Bracket Bolts | 55 N·m | 41 lb ft
Torque Rod-to-Frame Through Bolt | 55 N·m | 41 lb ft
Torque Rod-to-Torque Rod Bracket Through Bolt and Nut | 55 N·m | 41 lb ft
Upper Generator Adjustment Bolt | 23 N·m | 17 lb ft
Upper Rear Mounting Bracket Retaining Nuts | 55 N·m | 41 lb ft